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Site-Prep Checklist for a 3D Laser Scan
A little prep makes capture faster, safer, and more complete. Check each item before the scan crew arrives.
Before the scan
☐  Clear access to every area to be scanned (unlock doors, move what you can)
☐  Provide keys, badges, or an escort for secured / restricted rooms
☐  Confirm occupancy and available work hours (after-hours / weekends if needed)
☐  Identify any areas NOT to be scanned (privacy, security, tenant spaces)
☐  Flag hazards, confined spaces, and required PPE
☐  Note ceiling/roof, mechanical room, and above-ceiling access needs
☐  Point out mirrors, glass, and highly reflective surfaces
☐  Gather existing drawings or prior scans, if available
☐  Confirm parking / loading access for equipment
☐  Designate an on-site point of contact
Day of capture
☐  Walk the crew through the site and confirm scope
☐  Keep foot traffic to a minimum in active scan areas
☐  Leave temporary targets / control markers undisturbed
☐  Confirm any last-minute exclusions in writing
After capture
☐  Confirm the deliverable list, formats, and required LOA
☐  Set the review window and point of contact for questions
☐  Schedule any follow-up capture for areas that were inaccessible
Questions before your scan? CAD Construct LLC — cadconstructllc.com
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